# Adapter Specifications

|  | Intel® PRO/100+ Management Adapter
|  | Intel PRO/100 VE Desktop Adapters and Network Connections
|  | Intel PRO/100+ Server Adapter
|  | Intel PRO/100+ Dual Port Server Adapter
|  | Intel PRO/100 S Server Adapter

### Intel(R) PRO/100+ Management Adapter

Feature |  | Value
Bus Compatibility |  | PCI 2.2 specification, 32-bit
Media (cable) Connectors and Wiring |  | RJ45 Use Category 5 cabling at 100 Mbps Supports 100BASE TX Fast Ethernet
Data Rate Mode |  | 10 or 100 Mbps
Interrupt Levels |  | PCI: INTA
SRAM Transmit/Receive Buffer |  | 6 Kbytes
Power Requirements |  | 0.67 Watts @ 5.0VDC
Isolation Voltage |  | 200V RMS
Operating Temperature |  | 0 - 55 degrees C
Humidity |  | 10% - 90% non-condensing
Diagnostic LEDs |  | Activity/Link, 100 Mbps
Compliance & Certification |  | Safety -- UL FCC Class B CE & Immunity C-tick (Australian) BSMI (Taiwan)

Back to Top

### Intel® PRO/100 VE and VM Desktop Adapters and Network Connections

Feature |  | Value
Bus Compatibility |  | LAN on Motherboard: PCI 2.2 specification. LAN on Riser: CNR 1.0 specification. CNR Interfaces used: SMBus, LAN Connect Interface, LAN EEPROM.
Media (cable) Connectors and Wiring |  | RJ45 connector. Category 5 UTP cabling at 100 Mbps Supports 100BASE TX Fast Ethernet
Data Rate Mode |  | 10 or 100 Mbps
Interrupt Levels |  | PCI: INTA
SRAM Transmit/Receive Buffer |  | N/A (built-in to ICH2 chipset)
Power Requirements |  | 0.3 Watts @ 3.3VDC
Isolation Voltage |  | 200V RMS
Operating Temperature |  | 0 - 55 degrees C
Humidity |  | 10% - 90% non-condensing
Diagnostic LEDs |  | Activity/Link, 100 Mbps
Compliance & Certification |  | Safety -- UL FCC Class B CE & Immunity C-tick (Australian)

Back to Top

### Intel® PRO/100+ Server Adapter

Feature |  | Value
Bus Compatibility |  | PCI 2.2 specification, 32-bit
Media (cable) Connectors and Wiring |  | RJ45 Use Category 5 cabling at 100 Mbps Supports 100BASE TX Fast Ethernet
Data Rate Mode |  | 10 or 100 Mbps
Interrupt Levels |  | PCI: INTA
SRAM Transmit/Receive Buffer |  | 6 Kbytes
Power Requirements |  | 0.67 Watts @ 5.0VDC
Isolation Voltage |  | 200V RMS
Operating Temperature |  | 0 - 55 degrees C
Humidity |  | 10% - 90% non-condensing
Standards conformance |  | IEEE 802.3 IEEE 802.3ac IEEE 802.3z IEEE 802.3x IEEE 802.1p IEEE 802.1Q PCI 2.2 specification
Diagnostic LEDs |  | Activity/Link, 100 Mbps
Compliance & Certification |  | Safety -- UL FCC Class B CE & Immunity C-tick (Australian) BSMI (Taiwan)

Back to Top

### Intel® PRO/100+ Dual Port Server Adapter

Feature |  | Value
Bus Compatibility |  | PCI 2.1 specification, 32-bit (adapters with part numbers 715191-00x and 751110-00x).
Media (cable) Connectors and Wiring |  | RJ45 Use Category 5 cabling at 100 Mbps Supports 100BASE TX Fast Ethernet Standard
Data Rate Mode |  | 10 or 100 Mbps
Interrupt Levels |  | PCI: INTA, INTB
SRAM Transmit/Receive Buffer |  | 6 Kbytes per port
Power Requirements |  | 6.5 Watts @ +5VDC (715191-00x and 751110-00x)
Isolation Voltage |  | 200V RMS
Operating Temperature |  | 0 - 55 degrees C
Humidity |  | 10% - 90% non-condensing
Diagnostic LEDs |  | Activity, Link, 100 Mbps
Compliance & Certification |  | Safety -- UL FCC Class B CE & Immunity C-tick (Australian) BSMI (Taiwan)

Back to Top

### Intel® PRO/100 S Server Adapter

Feature |  | Value
Bus Compatibility |  | PCI 2.2 specification, 32-bit
Media (cable) Connectors and Wiring |  | RJ45 Use Category 5 cabling at 100 Mbps Supports 100BASE TX Fast Ethernet
Data Rate Mode |  | 10 or 100 Mbps
Interrupt Levels |  | PCI: INTA
SRAM Transmit/Receive Buffer |  | 6 Kbytes
Power Requirements |  | 1.73 Watts @ 5.0VDC
Isolation Voltage |  | 200V RMS
Operating Temperature |  | 0 - 55 degrees C
Humidity |  | 10% - 90% non-condensing
Diagnostic LEDs |  | Activity/Link, 100 Mbps
Compliance & Certification |  | Safety -- UL FCC Class B CE & Immunity C-tick (Australian) BSMI (Taiwan)

Back to Top