# Specifications

## General Specifications

> Type II: Model MBLA3300 (LAN only)

> Type II: Model MBLA3356 (Combo)

> Type III: Model MBLA3400C3 (LAN only)

> Type III: Model MBLA3456C3 (Combo)

> > Cable: 100Base-TX unshielded twisted pair for use on Category 5 (data grade) cabling; 10Base-T unshielded twisted pair (UTP)

> > Operating Distance: 328 ft (100 m)

> ### Ethernet Specifications:

> > Ethernet IEEE 802.3 for 10 Mbps, 802.3u for 100 Mbps

> > Type II/III CardBus PC Card

> > 10/100 Mbps full-duplex

> > Size: 3.37 in (86 mm) x 2.13 in (54.0 mm) x 0.20 in (5.0 mm) excluding adapter cable and network connection

> > Weight: 0.85 oz (24 g)

> ### Power Requirements:

> > MBLA3300/3400C3 3.3V DC, 52mA at 10 Mbps; 120mA at 100 Mbps; 7 - 19mA with LAN cable removed

> > MBLA3356/3456C3 3.3V DC, 96mA at 10 Mbps; 160mA at 100 Mbps; 7 - 19mA with LAN cable removed; modem only 225mA

> ### Power Management:

> > Supports ACPI and CardBus Power Management Specification

| NOTE: This adapter includes the smart power-down feature. By disconnecting the LAN cable from the adapter, Smart power down automatically reduces the power consumed by the PC card, extending battery life.

> ### Temperature Range:

> > Operating: 32°F to 131°F (0°C to 55°C)

> > Storage: -4°F to 149°F (-20°C to 65°C)

> > Humidity: 95% max. non-condensing

> ### LEDs:

> > Link integrity, transmission activity

> ### Certification:

> - FCC Code of Federal Regulations, Title 47, Part 15, Subpart B, Class A

> - CE Mark (EN 55022, Class A, EN50082)

> - C-Tick (Australia)

> - (Regional regulations vary by product--check the product datasheet for additional information.)

## Modem Specifications

> ### Data Modulation:

> - K56flex*/V.90 up to 56Kbps (subject to local regulations)

> - V.34 from 33,600 down to 2400 bps; V.32terbo at 19200 and 16800 bps

> - V.32bis at 14400, 12000, 9600, and 7200 bps, uncoded at 4800 bps

> - V.32 at 9600 bps, uncoded at 4800 bps

> - V.23 at 1200/75 and 75/1200 bps

> - V.22bis at 2400 bps

> - V.22 at 1200 bps; Bell 212A at 1200 bps

> ### Fax Modulation:

> - V.17 at 14400, 12000, 9600, 7200, and 4800 bps

> - V.29 at 9600, 7200, and 4800 bps

> - V.27ter at 4800 and 2400 bps

> ### Fax Support:

> > Group 3, EIA/TIA Class 1

> ### Error Control:

> > V.42 Error Control, MNP Levels 2-4 Error Detection

> ### Data Compression:

> > V.42bis (4:1) or MNP Level 5 (2:1)

> ### Command Set:

> > Hayes- and Microcom-compatible AT commands

> ### DTE Speeds:

> > 1200, 2400, 4800, 7200, 9600, 14400, 19200, 37400, 57600, and 115200 bps

> ### Certification:

> - FCC code of federal regulations, Title 47, Part 68

> - Industry Canada, C503 155VE8

> - CTR21 (Europe)

> - iDA (Singapore)

> - A-Tick Mark (Australia)

> - Telepermit (New Zealand)

> - (Regional regulations vary by product--check the product datasheet for additional information)